## int 13

| Interrups | Categories | Contents

Int 13/AH=00h - DISK - RESET DISK SYSTEM
Int 13/AH=01h - DISK - GET STATUS OF LAST OPERATION
Int 13/AH=02h - DISK - READ SECTOR(S) INTO MEMORY
Int 13/AH=03h - DISK - WRITE DISK SECTOR(S)
Int 13/AH=04h - DISK - VERIFY DISK SECTOR(S)
Int 13/AH=05h - FLOPPY - FORMAT TRACK
Int 13/AH=05h - FIXED DISK - FORMAT TRACK
Int 13/AH=05h - Future Domain SCSI BIOS - SEND SCSI MODE SELECT COMMAND
Int 13/AX=057Fh/SI=324Dh - 2M - FORMAT TRACK
Int 13/AH=06h - FIXED DISK - FORMAT TRACK AND SET BAD SECTOR FLAGS (XT,PORT)
Int 13/AH=06h - Future Domain SCSI BIOS - FORMAT DRIVE WITH BAD SECTOR MAPPING
Int 13/AH=06h - Adaptec AHA-154xA/Bustek BT-542 BIOS - IDENTIFY SCSI DEVICES
Int 13/AH=06h - V10DISK.SYS - READ DELETED SECTORS
Int 13/AH=07h - FIXED DISK - FORMAT DRIVE STARTING AT GIVEN TRACK (XT,PORT)
Int 13/AH=07h - Future Domain SCSI BIOS - FORMAT DRIVE
Int 13/AH=07h - V10DISK.SYS - WRITE DELETED SECTORS
Int 13/AH=08h - DISK - GET DRIVE PARAMETERS (PC,XT286,CONV,PS,ESDI,SCSI)
Int 13/AH=08h - V10DISK.SYS - SET FORMAT
Int 13/AX=0800h/DL=F0h - SecureDrive - INSTALLATION CHECK
Int 13/AH=09h - HARD DISK - INITIALIZE CONTROLLER WITH DRIVE PARAMETERS (AT,PS)
Int 13/AH=0Ah - HARD DISK - READ LONG SECTOR(S) (AT and later)
Int 13/AH=0Bh - HARD DISK - WRITE LONG SECTOR(S) (AT and later)
Int 13/AH=0Ch - HARD DISK - SEEK TO CYLINDER
Int 13/AH=0Dh - HARD DISK - RESET HARD DISKS
Int 13/AH=0Eh - HARD DISK - READ SECTOR BUFFER (XT only)
Int 13/AH=0Fh - HARD DISK - WRITE SECTOR BUFFER (XT only)
Int 13/AH=10h - HARD DISK - CHECK IF DRIVE READY
Int 13/AH=11h - HARD DISK - RECALIBRATE DRIVE
Int 13/AH=12h - HARD DISK - CONTROLLER RAM DIAGNOSTIC (XT,PS)
Int 13/AH=12h - Future Domain SCSI CONTROLLER - STOP SCSI DISK
Int 13/AH=12h - SyQuest - START/STOP SCSI DISK
Int 13/AH=13h - HARD DISK - DRIVE DIAGNOSTIC (XT,PS)
Int 13/AH=13h - SyQuest - READ DRIVE PARAMATERS (for DOS 5+)
Int 13/AH=14h - HARD DISK - CONTROLLER INTERNAL DIAGNOSTIC
Int 13/AH=15h - DISK - GET DISK TYPE (XT 1986/1/10 or later,XT286,AT,PS)
Int 13/AH=16h - FLOPPY DISK - DETECT DISK CHANGE (XT 1986/1/10 or later,XT286,AT,PS)
Int 13/AH=17h - FLOPPY DISK - SET DISK TYPE FOR FORMAT (AT,PS)
Int 13/AX=1700h - Future Domain SCSI CONTROLLER - GET INQUIRY INFO FROM SCSI DEVICE
Int 13/AH=18h - DISK - SET MEDIA TYPE FOR FORMAT (AT model 3x9,XT2,XT286,PS)
Int 13/AH=18h - Future Domain SCSI BIOS - GET SCSI CONTROLLER INFORMATION
Int 13/AH=18h/CX=5055h - PU_1700.COM - INSTALLATION CHECK
Int 13/AH=18h/CX=D2C9h - XDF.COM - API
Int 13/AH=19h - FIXED DISK - PARK HEADS ON ESDI DRIVE (XT286,PS)
Int 13/AH=19h - Future Domain SCSI CONTROLLER - REINITIALIZE DRIVE
Int 13/AH=1Ah - ESDI FIXED DISK - FORMAT UNIT (PS)
Int 13/AH=1Ah - Future Domain SCSI CONTROLLER - GET SCSI PARTIAL MEDIUM CAPACITY
Int 13/AH=1Bh - ESDI FIXED DISK - GET MANUFACTURING HEADER
Int 13/AH=1Bh - Future Domain SCSI CONTROLLER - GET POINTER TO SCSI DISK INFO BLOCK
Int 13/AH=1Ch - Future Domain SCSI CONTROLLER - GET POINTER TO FREE CONTROLLER RAM
Int 13/AH=1Ch - ESDI FIXED DISK - ???
Int 13/AX=1C08h - ESDI FIXED DISK - GET COMMAND COMPLETION STATUS
Int 13/AX=1C09h - ESDI FIXED DISK - GET DEVICE STATUS
Int 13/AX=1C0Ah - ESDI FIXED DISK - GET DEVICE CONFIGURATION
Int 13/AX=1C0Bh - ESDI FIXED DISK - GET ADAPTER CONFIGURATION
Int 13/AX=1C0Ch - ESDI FIXED DISK - GET POS INFORMATION
Int 13/AX=1C0Dh - ESDI FIXED DISK - ???
Int 13/AX=1C0Eh - ESDI FIXED DISK - TRANSLATE RBA TO ABA
Int 13/AX=1C0Fh - ESDI FIXED DISK - ???
Int 13/AX=1C12h - ESDI FIXED DISK - ???
Int 13/AH=1Dh - IBMCACHE.SYS - CACHE STATUS
Int 13/AH=1Fh - SyQuest - DOOR LATCH/DOOR BUTTON DETECT
Int 13/AH=20h - DISK - ??? (Western Digital Super BIOS)
Int 13/AH=20h - Compaq, ATAPI Removable Media Device - GET CURRENT MEDIA FORMAT
Int 13/AH=20h - QUICKCACHE II v4.20 - DISMOUNT
Int 13/AH=21h - HARD DISK - PS/1 and newer PS/2 - READ MULTIPLE DISK SECTORS
Int 13/AH=21h - QUICKCACHE II v4.20 - FLUSH CACHE
Int 13/AH=22h - HARD DISK - PS/1 and newer PS/2 - WRITE MULTIPLE DISK SECTORS
Int 13/AH=22h - QUICKCACHE II v4.20 - ENABLE/DISABLE CACHE
Int 13/AH=23h - HARD DISK - PS/1 and newer PS/2 - SET CONTROLLER FEATURES REGISTER
Int 13/AH=23h - QUICKCACHE II v4.20 - GET ??? ADDRESS
Int 13/AH=24h - HARD DISK - PS/1 and newer PS/2 - SET MULTIPLE MODE
Int 13/AH=24h - QUICKCACHE II v4.20 - SET SECTORS
Int 13/AH=25h - HARD DISK - PS/1 and newer PS/2 - IDENTIFY DRIVE
Int 13/AH=25h - QUICKCACHE II v4.20 - SET FLUSH INTERVAL
Int 13/AH=26h - QUICKCACHE II v4.20 - UNINSTALL
Int 13/AH=27h/BX=0000h - QUICKCACHE II v4.20 - INSTALLATION CHECK
Int 13/AH=28h - QUICKCACHE II v4.20 - SET AUTOMATIC DISMOUNT
Int 13/AH=29h - QUICKCACHE II v4.20 - NOP
Int 13/AH=2Ah - QUICKCACHE II v4.20 - SET BUFFER SIZE
Int 13/AH=2Bh - QUICKCACHE II v4.20 - DRIVE ACCESS SOUNDS
Int 13/AH=2Ch - QUICKCACHE II v4.20 - SET BUFFERED WRITES
Int 13/AH=2Dh - QUICKCACHE II v4.20 - SET BUFFERED READ
Int 13/AH=2Eh - QUICKCACHE II v4.20 - SET FLUSH COUNT
Int 13/AH=2Fh - QUICKCACHE II v4.20 - FORCE IMMEDIATE INCREMENTAL FLUSH
Int 13/AH=30h - QUICKCACHE II v4.20 - GET INFO
Int 13/AH=31h - QUICKCACHE II v4.20 - RESERVE MEMORY
Int 13/AH=32h - QUICKCACHE II v4.20 - ENABLE CACHING FOR SPECIFIC DRIVE
Int 13/AH=33h - QUICKCACHE II v4.20 - DISABLE CACHING FOR SPECIFIC DRIVE
Int 13/AH=34h - QUICKCACHE II v4.20 - SECTOR LOCKING
Int 13/AH=35h - QUICKCACHE II v4.20 - SET LOCK POOL SIZE
Int 13/AH=36h - QUICKCACHE II v4.20 - SET TRACE BUFFER SIZE
Int 13/AH=37h - QUICKCACHE II v4.20 - SET BUFFERED READS FOR SPECIFIC DRIVE
Int 13/AH=38h - QUICKCACHE II v4.20 - SET BUFFERED WRITES FOR SPECIFIC DRIVE
Int 13/AH=39h - QUICKCACHE II v4.20 - SET READ BUFFER SIZE FOR SPECIFIC DRIVE
Int 13/AH=3Ah - QUICKCACHE II v4.20 - SET WRITE BUFFER SIZE FOR SPECIFIC DRIVE
Int 13/AH=3Bh - QUICKCACHE II v4.20 - ENABLE/DISABLE ???
Int 13/AH=3Ch - QUICKCACHE II v4.20 - ENABLE/DISABLE ???
Int 13/AH=3Dh - QUICKCACHE II v4.20 - ENABLE/DISABLE CYLINDER FLUSH FOR DRIVE
Int 13/AH=3Eh - QUICKCACHE II v4.20 - SET SINGLE-SECTOR BONUS
Int 13/AH=3Fh - QUICKCACHE II v4.20 - SET BONUS THRESHOLD
Int 13/AH=40h - QUICKCACHE II v4.20 - SET sticky_max
Int 13/AH=41h/BX=55AAh - IBM/MS INT 13 Extensions - INSTALLATION CHECK
Int 13/AH=41h - QUICKCACHE II v4.20 - SAVE/RESTORE ???
Int 13/AH=42h - IBM/MS INT 13 Extensions - EXTENDED READ
Int 13/AX=4257h/DX=1234h - Beame&Whiteside BWLPD - INSTALLATION CHECK
Int 13/AH=43h - IBM/MS INT 13 Extensions - EXTENDED WRITE
Int 13/AH=44h - IBM/MS INT 13 Extensions - VERIFY SECTORS
Int 13/AH=45h - IBM/MS INT 13 Extensions - LOCK/UNLOCK DRIVE
Int 13/AH=46h - IBM/MS INT 13 Extensions - EJECT MEDIA
Int 13/AH=47h - IBM/MS INT 13 Extensions - EXTENDED SEEK
Int 13/AH=48h - IBM/MS INT 13 Extensions - GET DRIVE PARAMETERS
Int 13/AH=49h - IBM/MS INT 13 Extensions - EXTENDED MEDIA CHANGE
Int 13/AH=4Ah - Bootable CD-ROM - INITIATE DISK EMULATION
Int 13/AX=4B00h - Bootable CD-ROM - TERMINATE DISK EMULATION
Int 13/AX=4B01h - Bootable CD-ROM - GET STATUS
Int 13/AH=4Ch - Bootable CD-ROM - INITIATE DISK EMULATION AND BOOT
Int 13/AX=4D00h - Bootable CD-ROM - RETURN BOOT CATALOG
Int 13/AH=4Eh - IBM/MS INT 13 Extensions v2.1+ - SET HARDWARE CONFIGURATION
Int 13/AX=5001h - Enhanced Disk Drive Spec v3.0 - SEND PACKET COMMAND
Int 13/AX=5001h - VIRUS - Andropinis - INSTALLATION CHECK
Int 13/AX=5342h/CX=0001h - ScanBoot - INSTALLATION CHECK
Int 13/AX=5501h - Seagate ST01/ST02 - Inquiry
Int 13/AX=5502h - Seagate ST01/ST02 - RESERVED
Int 13/AX=5503h - Seagate ST01/ST01 - Set Device Type Qualifier (DTQ)
Int 13/AX=5504h - Seagate - ??? - RETURN IDENTIFICATION
Int 13/AX=5504h - Seagate ST01/ST02 - RETURN IDENTIFICATION
Int 13/AX=5505h - Seagate - ??? - PARK HEADS
Int 13/AX=5505h - Seagate ST01/ST02 - PARK HEADS
Int 13/AX=5506h - Seagate ST01/ST02 - SCSI Bus Parity
Int 13/AX=5507h - Seagate ST01/ST02 - RESERVED FUNCTIONS
Int 13/AX=5514h - Seagate - ???
Int 13/AX=5515h - Seagate - PARK HEADS???
Int 13/AH=59h - SyQuest - Generic SCSI pass through
Int 13/AH=70h - Priam EDVR.SYS DISK PARTITIONING SOFTWARE???
Int 13/AH=75h - ???
Int 13/AH=76h - ???
Int 13/AX=7B00h - NOW! v3.05 - GET INFORMATION
Int 13/AX=7B01h - NOW! v3.05 - ???
Int 13/AX=7B02h - NOW! v3.05 - SET INFORMATION
Int 13/AX=7B03h - NOW! v3.05 - ???
Int 13/AX=7B04h - NOW! v3.05 - ???
Int 13/AX=7B05h - NOW! v3.05 - GET DISK ACCESSES???
Int 13/AX=7B06h - NOW! v3.05 - GET ???
Int 13/AX=7B07h - NOW! v3.05 - GET ???
Int 13/AX=7B08h - NOW! v3.05 - ???
Int 13/AH=80h/CX=6572h - FAST! v4.02+ - API
Int 13/AX=8001h/CX=6572h - FAST! v4.02+ - GET CACHE INFORMATION
Int 13/AX=8006h/CX=6572h - FAST! v4.02+ - INSTALLATION CHECK
Int 13/AX=8007h/CX=6572h - FAST! v4.02+ - UNHOOK INTERRUPTS
Int 13/AH=81h/SI=4358h - Super PC-Kwik v3.20+ - ???
Int 13/AH=82h/SI=4358h - Super PC-Kwik v3.20+ - ???
Int 13/AH=83h/SI=4358h - Super PC-Kwik v3.20+ - ???
Int 13/AH=84h/SI=4358h - Super PC-Kwik v3.20+ - ???
Int 13/AH=85h/SI=4358h - Super PC-Kwik v3.20+ - ???
Int 13/AH=86h/SI=4358h - Super PC-Kwik v4.00+ - ???
Int 13/AH=87h/SI=4358h - Super PC-Kwik v4.00+ - ???
Int 13/AH=88h/SI=4358h - Super PC-Kwik v4.00+ - ???
Int 13/AH=89h/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=8Ah/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AX=8EEDh - HyperDisk v4.01+ - ???
Int 13/AX=8EEEh - HyperDisk v4.01+ - ???
Int 13/AX=8EEFh - HyperDisk v4.01+ - ???
Int 13/AH=92h/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=93h/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=94h/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=95h/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=96h/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=97h/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=98h/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=99h/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=9Ah/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=9Bh/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=9Ch/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=9Dh/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=A0h/SI=4358h - Super PC-Kwik v3.20+ - GET RESIDENT CODE SEGMENT
Int 13/AH=A1h/SI=4358h - Super PC-Kwik v3.20+ - FLUSH CACHE
Int 13/AH=A2h/SI=4358h - Super PC-Kwik v3.20+ - ???
Int 13/AH=A3h/SI=4358h - Super PC-Kwik v5.10+ - DISABLE CACHE
Int 13/AH=A4h/SI=4358h - Super PC-Kwik v5.10+ - ENABLE CACHE
Int 13/AH=A5h/SI=4358h - Super PC-Kwik v5.10+ - PROGRAM TERMINATION NOTIFICATION
Int 13/AH=A6h/SI=4358h - Super PC-Kwik v5.10+ - PROGRAM LOAD NOTIFICATION
Int 13/AH=A7h/SI=4358h - Super PC-Kwik 5.1 - ???
Int 13/AX=A759h - Novell DOS 7 - SDRes v27.03 - ???
Int 13/AH=A8h/SI=4358h - Super PC-Kwik 5.1 - ???
Int 13/AH=A9h/SI=4358h - Super PC-Kwik 5.1 - EXITCODE RETRIEVAL NOTIFICATION
Int 13/AH=AAh/SI=4358h - Super PC-Kwik v4+ - ???
Int 13/AH=ABh/SI=4358h - Super PC-Kwik v4+ - ???
Int 13/AH=ACh/SI=4358h - Super PC-Kwik v4+ - ???
Int 13/AH=ADh - Priam HARD DISK CONTROLLER???
Int 13/AH=ADh/SI=4358h - Super PC-Kwik v4+ - ???
Int 13/AH=AEh/SI=4358h - Super PC-Kwik v5.10+ - ???
Int 13/AH=B0h/SI=4358h - Super PC-Kwik v3.20+ - ???
Int 13/AX=BF00h - Mylex/Adaptec??? - ???
Int 13/AX=E000h - XBIOS - COMMAND
Int 13/AX=EC00h - VIRUS - Tiso - INSTALLATION CHECK
Int 13/AH=EEh - SWBIOS - SET 1024-CYLINDER FLAG
Int 13/AH=EFh - Ontrack Drive Rocket - SET CYLINDER OFFSET
Int 13/AH=F2h - VIRUS - Neuroquila - INSTALLATION CHECK
Int 13/AH=F9h - SWBIOS - INSTALLATION CHECK
Int 13/AH=FAh/DX=5945h - PC Tools v8+ VSAFE, VWATCH - API
Int 13/AX=FD50h - VIRUS - Predator - INSTALLATION CHECK
Int 13/AH=FEh - SWBIOS - GET EXTENDED CYLINDER COUNT
Int 13/AH=FFh - EZ-Drive - INSTALLATION CHECK
Int 13/AH=FFh - IBM SurePath BIOS - Officially Private Function
Int 13/AX=FFFFh/BH=AAh - UNIQUE UX Turbo Utility - SET TURBO MODE

| Interrups | Categories | Contents

Shopping | Forum | EMail | Index | Home |

Rate My Photo