INT 13H - Wikipedia, the free encyclopedia

# INT 13H

From Wikipedia, the free encyclopedia

| This article needs additional citations for verification. Please help improve this article by adding citations to reliable sources. Unsourced material may be challenged and removed. (September 2010)

INT 13H, INT 13h, or INT 19 is shorthand for BIOS interrupt call 13hex, the 20th interrupt vector in an x86-based computer system. The BIOS typically sets up a real mode interrupt handler at this vector that provides sector-based hard disk and floppy disk read and write services using cylinder-head-sector (CHS) addressing.

INT is an x86 instruction that triggers a software interrupt, and 13hex vector passed to the instruction (interrupts start at zero, and are labeled with hexadecimal values).

## [edit] Overview

See also: Enhanced BIOS

Under real mode operating systems, such as MS-DOS, calling INT 13h would jump into the computer's ROM-BIOS code for low-level disk services, which would carry out physical sector-based disk read or write operations for the program. In MS-DOS, it serves as the low-level interface for the built-in block device drivers for hard and floppy disks in the DOS-BIOS, which, through INT 25h and INT 26h, provides absolute disk read/write functions for logical sectors to the FAT file system driver in the DOS kernel, which handles file-related requests through MS-DOS API (INT 21h) functions.

Under protected mode operating systems, such as Microsoft Windows NT derivatives (e.g. NT4, 2000, XP, and Server 2003) and Linux with dosemu, the OS intercepts the call and passes it to the operating system's native disk I/O mechanism. Windows 9x and Windows for Workgroups 3.11 also bypass BIOS routines when using 32-bit File Access.

The original BIOS real-mode INT 13h interface supports drives of sizes up to about 504 MB using what is commonly referred to as physical CHS addressing. This limit originates from the hardware interface of the IBM PC/XT disk hardware. The BIOS used the cylinder-head-sector (CHS) address given in the INT 13h call, and transferred it directly to the hardware interface.

This interface was later extended to support addressing of up to exactly 8064 MB using what is commonly referred to as logical CHS addressing. This limit originates from a combination of the register value based calling convention used in the INT 13h interface, and the goal of maintaining backward compatibility. There were originally a number of BIOSes that offered incompatible versions of this interface, but eventually the computer industry standardized on the interface developed in the Microid Research ("MR BIOS") in 1989. This limit uses 1024 cylinders, 256 heads, 63 sectors, and 512 byte blocks, giving roughly 7.875 GB of addressing (1024 * 256 * 63 * 512).

To support even larger addressing modes, an interface known as INT 13h Extensions was introduced by Western Digital and Phoenix Technologies as part of BIOS Enhanced Disk Drive Services (EDD) standard.[citation needed] It uses 64-bit logical block addressing (LBA) which allows addressing up to 8 ZiB (the drive can also support 28-bit or 48-bit LBA which allows up to 128 GiB or 128 PiB respectively, assuming a 512-byte sector/block size). This is a packet interface, because it uses a pointer to a packet of information rather than the register based calling convention of the original INT 13h interface. This packet is a data structure that contains an interface version, data size, and LBAs.

All versions of MS-DOS, including MS-DOS 7, and Windows 95 contain a bug that prevents booting hard disks with 256 heads (register value 0xFF),[citation needed] so many modern BIOS maps the drives to have at most 255 heads. Also some cache drivers will flush their buffers when detecting that MS-DOS is bypassed by applications that directly issues INT 13h requests. AMI BIOSes from around 1990-1991 trash word unaligned buffers. Some MS-DOS and TSR programs clobber interrupt enabling and registers so PC-DOS and MS-DOS install their own filters to prevent this.[1]

## [edit] List of INT 13h services

### [edit] Drive Table

DL = 00h | 1st floppy disk ( "drive A:" )
DL = 01h | 2nd floppy disk ( "drive B:" )
DL = 80h | 1st hard disk
DL = 81h | 2nd hard disk

### [edit] Function Table

AH = 00h |  | Reset Disk Drives
AH = 01h |  | Get Status of Last Drive Operation
AH = 02h |  | Read Sectors From Drive
AH = 03h |  | Write Sectors To Drive
AH = 04h |  | Verify Sectors
AH = 05h |  | Format Track
AH = 06h |  | Format Track Set Bad Sector Flags
AH = 07h |  | Format Drive starting at Track
AH = 08h |  | Read Drive Parameters
AH = 09h | HD | Initialize Disk Controller
AH = 0Ah | HD | Read Long Sectors From Drive
AH = 0Bh | HD | Write Long Sectors To Drive
AH = 0Ch | HD | Move Drive Head To Cylinder
AH = 0Dh | HD | Reset Disk Drives
AH = 0Eh | PS/2 | Controller Read Test
AH = 0Fh | PS/2 | Controller Write Test
AH = 10h | HD | Test Whether Drive Is Ready
AH = 11h | HD | Recalibrate Drive
AH = 12h | PS/2 | Controller RAM Test
AH = 13h | PS/2 | Drive Test
AH = 14h | HD | Controller Diagnostic
AH = 15h |  | Read Drive Type
AH = 16h | FD | Detect Media Change
AH = 17h | FD | Set Media Type For Format ( used by DOS versions <= 3.1 )
AH = 18h | FD | Set Media Type For Format ( used by DOS versions >= 3.2 )
AH = 19h |  | Park Heads
AH = 41h | EXT | Test Whether Extensions Are Available
AH = 42h | EXT | Read Sectors From Drive
AH = 43h | EXT | Write Sectors To Drive
AH = 44h | EXT | Verify Sectors
AH = 45h | EXT | Lock/Unlock Drive
AH = 46h | EXT | Eject Drive
AH = 47h | EXT | Move Drive Head To Sector
AH = 48h | EXT | Read Drive Parameters
AH = 49h | EXT | Detect Media Change

If the second column is empty then the function may be used both for floppy and hard disk.

- FD: for floppy disk only.
- HD: for hard disk only.
- PS/2: for hard disk on PS/2 system only.
- EXT: part of the Int 13h Extensions which were written in the 1990s to support hard drives with more than 8 GB.

### [edit] INT 13h AH=00h: Reset Disk Drive

Parameters:

AH | 00h
DL | Drive

Results:

CF | Set on error

### [edit] INT 13h AH=01h: Get Status of Last Drive Operation

Parameters:

AH | 01h
DL | Drive$

$Bit 7=0 for floppy drive, bit 7=1 for fixed drive

Results:

AL

Return Code

00h | Success
01h | Invalid Command
02h | Cannot Find Address Mark
03h | Attempted Write On Write Protected Disk
04h | Sector Not Found
05h | Reset Failed
06h | Disk change line 'active'
07h | Drive parameter activity failed
08h | DMA overrun
09h | Attempt to DMA over 64kb boundary
0Ah | Bad sector detected
0Bh | Bad cylinder (track) detected
0Ch | Media type not found
0Dh | Invalid number of sectors
0Eh | Control data address mark detected
0Fh | DMA out of range
10h | CRC/ECC data error
11h | ECC corrected data error
20h | Controller failure
40h | Seek failure
80h | Drive timed out, assumed not ready
AAh | Drive not ready
BBh | Undefined error
CCh | Write fault
E0h | Status error
FFh | Sense operation failed

CF | Set On Error, Clear If No Error

### [edit] INT 13h AH=02h: Read Sectors From Drive

Parameters:

AH | 02h
AL | Sectors To Read Count
CH | Track
CL | Sector
DH | Head
DL | Drive
ES:BX | Buffer Address Pointer

Results:

CF | Set On Error, Clear If No Error
AH | Return Code
AL | Actual Sectors Read Count

Remarks:
Register CX contains both the cylinder number (10 bits, possible values are 0 to 1023) and the sector number (6 bits, possible values are 1 to 63):

    CX =       ---CH--- ---CL---
    cylinder : 76543210 98
    sector   :            543210

Examples of translation:

    CX := ( ( cylinder and 255 ) shl 8 ) or ( ( cylinder and 768 ) shr 2 ) or sector;
    cylinder := ( (CX and 0xFF00) shr 8 ) or ( (CX and 0xC0) shl 2)
    sector := CX and 63;

Addressing of Buffer should guarantee that the complete buffer is inside the given segment, i.e. ( BX + size_of_buffer ) <= 10000h. Otherwise the interrupt may fail with some BIOS or hardware versions.
Example: Assume you want to read 16 sectors (= 2000h bytes) and your buffer starts at memory address 4FF00h. Utilizing memory segmentation, there are different ways to calculate the register values, e.g.:

    ES = segment         = 4F00h
    BX = offset          =  0F00h
    sum = memory address = 4FF00h
    would be a good choice because 0F00h + 2000h = 2F00h <= 10000h
    ES = segment         = 4000h
    BX = offset          =  FF00h
    sum = memory address = 4FF00h
    would not be a good choice because FF00h + 2000h = 11F00h > 10000h

Function 02h of interrupt 13h may only read sectors of the first 16,450,560 sectors of your hard drive, to read sectors beyond the 8 GB limit you should use function 42h of Int 13h Extensions. Another alternate may be DOS interrupt 25h which reads sectors within a partition.

### [edit] INT 13h AH=03h: Write Sectors To Drive

Parameters:

AH | 03h
AL | Sectors To Write Count
CH | Track
CL | Sector
DH | Head
DL | Drive
ES:BX | Buffer Address Pointer

Results:

CF | Set On Error, Clear If No Error
AH | Return Code
AL | Actual Sectors Written Count

### [edit] INT 13h AH=04h: Verify Sectors From Drive

Parameters:

AH | 04h
AL | Sectors To Verify Count
CH | Track
CL | Sector
DH | Head
DL | Drive
ES:BX | Buffer Address Pointer

Results:

CF | Set On Error, Clear If No Error
AH | Return Code
AL | Actual Sectors Verified Count

### [edit] INT 13h AH=05h: Format Track

Parameters:

AH | 05h
AL | Sectors To Format Count
CH | Track
CL | Sector
DH | Head
DL | Drive
ES:BX | Buffer Address Pointer$

$4-byte address field (applies to PC/XT 286,AT, PS/1 and PS/2)

Byte | Meaning | Allowable Values
1 | Track |
2 | Head |
3 | Sector |
4 | Bytes/Sector | 0=128, 1-256, 2-512, 3-1024

Results:

CF | Set On Error, Clear If No Error
AH | Return Code

### [edit] INT 13h AH=06h: Format Track Set Bad Sector Flags

Parameters:

AH | 06h
AL | Interleave
CH | Track
CL | Sector
DH | Head
DL | Drive

Results:

CF | Set On Error, Clear If No Error
AH | Return Code

### [edit] INT 13h AH=07h: Format Track Set Bad Sector Flags

Parameters:

AH | 07h
AL | Interleave
CH | Track
CL | Sector
DH | Head
DL | Drive

Results:

CF | Set On Error, Clear If No Error
AH | Return Code

### [edit] INT 13h AH=08h: Read Drive Parameters

Parameters:

Registers
AH | 08h = function number for read_drive_parameters
DL | drive index (e.g. 1st HDD = 80h)
ES:DI[2] | set to 0000h:0000h to work around some buggy BIOS

Results:

CF | Set On Error, Clear If No Error
AH | Return Code
DL | number of hard disk drives
DH[2] | logical last index of heads = number_of - 1 (because index starts with 0)
CX | [7:6] [15:8][2] logical last index of cylinders = number_of - 1 (because index starts with 0) [5:0][2] logical last index of sectors per track = number_of (because index starts with 1)
BL[2] | drive type (only AT/PS2 floppies)
ES:DI[2] | pointer to drive parameter table (only for floppies)

Remarks:
Logical values of function 08h may/should differ from physical CHS values of function 48h.
Result register CX contains both cylinders and sector/track values, see remark of function 02h.

### [edit] INT 13h AH=09h: Init Drive Pair Characteristics

Parameters:

AH | 09h
DL | Drive

Results:

CF | Set On Error, Clear If No Error
AH | Return Code

### [edit] INT 13h AH=0Ah: Read Long Sectors From Drive

The only difference between this function and function 02h (see above) is that function 0Ah reads 516 bytes per sector instead of only 512. The last 4 bytes contains the Error Correction Code (ECC), a checksum of sector data.

### [edit] INT 13h AH=41h: Check Extensions Present

Parameters:

Registers
AH | 41h = function number for extensions check[3]
DL | drive index (e.g. 1st HDD = 80h)
BX | 55AAh

Results:

CF | Set On Not Present, Clear If Present
AH | Error Code or Major Version Number
BX | AA55h
CX | Interface support bitmask: 1 - Device Access using the packet structure 2 - Drive Locking and Ejecting 4 - Enhanced Disk Drive Support (EDD)

### [edit] INT 13h AH=42h: Extended Read Sectors From Drive

Parameters:

Registers
AH | 42h = function number for extended read
DL | drive index (e.g. 1st HDD = 80h)
DS:SI | segment:offset pointer to the DAP, see below

DAP : Disk Address Packet
offset range | size | description
00h | 1 byte | size of DAP = 16 = 10h
01h | 1 byte | unused, should be zero
02h..03h | 2 bytes | number of sectors to be read, (some Phoenix BIOSes are limited to a maximum of 127 sectors)
04h..07h | 4 bytes | segment:offset pointer to the memory buffer to which sectors will be transferred (note that x86 is little-endian: if declaring the segment and offset separately, the offset must be declared before the segment)
08h..0Fh | 8 bytes | absolute number of the start of the sectors to be read (1st sector of drive has number 0)

Results:

CF | Set On Error, Clear If No Error
AH | Return Code

### [edit] INT 13h AH=48h: Extended Read Drive Parameters

Parameters:

Registers
AH | 48h = function number for extended_read_drive_parameters
DL | drive index (e.g. 1st HDD = 80h)
DS:SI | segment:offset pointer to Result Buffer, see below

Result Buffer
offset range | size | description
00h..01h | 2 bytes | size of Result Buffer = 30 = 1Eh
02h..03h | 2 bytes | information flags
04h..07h | 4 bytes | physical number of cylinders = last index + 1 (because index starts with 0)
08h..0Bh | 4 bytes | physical number of heads = last index + 1 (because index starts with 0)
0Ch..0Fh | 4 bytes | physical number of sectors per track = last index (because index starts with 1)
10h..17h | 8 bytes | absolute number of sectors = last index + 1 (because index starts with 0)
18h..19h | 2 bytes | bytes per sector
1Ah..1Dh | 4 bytes | optional pointer to Enhanced Disk Drive (EDD) configuration parameters which may be used for subsequent interrupt 13h Extension calls (if supported)

Results:

CF | Set On Error, Clear If No Error
AH | Return Code

Remark: Physical CHS values of function 48h may/should differ from logical values of function 08h.

## [edit] See also

- INT 10H
- BIOS interrupt call
- Cylinder-head-sector
- INT (x86 instruction)
- DPMI (DOS Protected Mode Interface)

## [edit] References

1. ^ ctyme.com - DISK - READ SECTOR(S) INTO MEMORY
2. ^ a b c d e f ctyme.com - DISK - GET DRIVE PARAMETERS (PC,XT286,CONV,PS,ESDI,SCSI)
3. ^ ctyme.com - IBM/MS INT 13 Extensions - INSTALLATION CHECK

## [edit] External links

- BIOS Interrupt 13h Extensions
- Ralf Brown's comprehensive Interrupt List
- Norton Guide about int 13h, ah = 00h .. 1ah

Retrieved from "http://en.wikipedia.org/w/index.php?title=INT_13H&oldid=474528966"
Categories:

- IBM PC compatibles
- BIOS
- Interrupts

Hidden categories:

- Articles needing additional references from September 2010
- All articles needing additional references
- All articles with unsourced statements
- Articles with unsourced statements from February 2012
- Articles with unsourced statements from July 2011

##### Personal tools

- Log in / create account

##### Interaction

- Help
- About Wikipedia
- Community portal
- Recent changes
- Contact Wikipedia

##### Toolbox

- What links here
- Related changes
- Upload file
- Special pages
- Permanent link
- Cite this page

##### Print/export

- Create a book
- Download as PDF
- Printable version

##### Languages

- Español
- Bahasa Indonesia