## int 1A

| Interrups | Categories | Contents

Int 1A/AH=00h - TIME - GET SYSTEM TIME
Int 1A/AH=01h - TIME - SET SYSTEM TIME
Int 1A/AH=02h - TIME - GET REAL-TIME CLOCK TIME (AT,XT286,PS)
Int 1A/AH=02h - Tandy 2000 - TIME - GET DATE AND TIME
Int 1A/AH=03h - TIME - SET REAL-TIME CLOCK TIME (AT,XT286,PS)
Int 1A/AH=03h - Tandy 2000 - TIME - SET DATE AND TIME
Int 1A/AH=04h - TIME - GET REAL-TIME CLOCK DATE (AT,XT286,PS)
Int 1A/AH=04h - Sperry PC - GET REAL-TIME CLOCK DATE
Int 1A/AH=04h/CX=4555h - CheckIt Year 2000 Fix v2.06 - INSTALLATION CHECK
Int 1A/AH=05h - TIME - SET REAL-TIME CLOCK DATE (AT,XT286,PS)
Int 1A/AH=05h - Sperry PC - SET REAL-TIME CLOCK DATE
Int 1A/AH=06h - TIME - SET ALARM (AT,XT286,PS)
Int 1A/AH=07h - TIME - CANCEL ALARM (AT,XT286,PS)
Int 1A/AH=08h - TIME - SET RTC ACTIVATED POWER ON MODE (CONVERTIBLE)
Int 1A/AH=09h - TIME - READ RTC ALARM TIME AND STATUS (CONV,PS30)
Int 1A/AH=0Ah - TIME - READ SYSTEM-TIMER DAY COUNTER (XT2,PS)
Int 1A/AH=0Bh - TIME - SET SYSTEM-TIMER DAY COUNTER (XT2,PS)
Int 1A/AH=0Ch - TIME - SET RTC DATE/TIME ACTIVATED POWER-ON MODE (IBM)
Int 1A/AH=0Dh - TIME - RESET RTC DATE/TIME ACTIVATED POWER-ON MODE (IBM)
Int 1A/AH=0Eh - TIME - GET RTC DATE/TIME ALARM AND STATUS (IBM)
Int 1A/AH=0Fh - TIME - INITIALIZE REAL-TIME CLOCK
Int 1A/AH=10h - NEC PC-9800 series - PRINTER - INITIALIZE
Int 1A/AX=1000h - NEC PC-9800 series - INSTALLATION CHECK
Int 1A/AH=11h - NEC PC-9800 series - PRINTER - OUTPUT CHARACTER
Int 1A/AH=12h - NEC PC-9800 series - PRINTER - SENSE STATUS
Int 1A/AX=3601h - WORD PERFECT v5.0 Third Party Interface - INSTALLATION CHECK
Int 1A/AX=6108h - SNAP.EXE 3.2+ - SNAP_SENDWITHREPLY - SEND MSG AND GET REPLY
Int 1A/AX=6205h - SNAP.EXE 3.2+ - SNAP_SENDNOREPLY - SEND MSG, DON'T AWAIT REPLY
Int 1A/AX=6308h - SNAP.EXE 3.2+ - SNAP_BEGINCONV - BEGIN CONVERSATION
Int 1A/AX=6405h - SNAP.EXE 3.2+ - SNAP_ENDCONV - END CONVERSATION
Int 1A/AX=6900h - SNAP.EXE 3.2+ - SNAP_DATASEG - GET RESIDENT DATA SEGMENT
Int 1A/AX=6A01h - SNAP.EXE 3.2+ - SNAP_ALLOC - ALLOCATE BUFFER IN SNAP DATA SEGMENT
Int 1A/AX=6B01h - SNAP.EXE 3.2+ - SNAP_FREE - DEALLOCATE BUFFER IN SNAP DATA SEGMENT
Int 1A/AX=6C04h - SNAP.EXE 3.2+ - SNAP_COPYTO - COPY DATA TO RESIDENT SNAP PACKAGE
Int 1A/AX=6D04h - SNAP.EXE 3.2+ - SNAP_COPYFROM - COPY DATA FROM RESIDENT SNAP PACKAGE
Int 1A/AX=6E01h - SNAP.EXE 3.2+ - SNAP_SETDEBUG - SET ???
Int 1A/AX=6F01h - SNAP.EXE 3.2+ - SNAP_CHKINSTALL - INSTALLATION CHECK
Int 1A/AX=7002h - SNAP.EXE 3.2+ - SNAP_SETANCHOR
Int 1A/AX=7101h - SNAP.EXE 3.2+ - SNAP_GETANCHOR
Int 1A/AX=7202h - SNAP.EXE 3.2+ - SNAP_SETCONVPARMS - SET CONVERSATION PARAMETERS
Int 1A/AX=7302h - SNAP.EXE 3.2+ - SNAP_CLIENTVERSION - ???
Int 1A/AX=7400h - SNAP.EXE 3.2+ - SNAP_VERSION - GET VERSION
Int 1A/AH=75h - SNAP.EXE 3.2+ - SNAP_NOP - ???
Int 1A/AH=76h - SNAP.EXE 3.2+ - SNAP_802_5 - ???
Int 1A/AH=77h - SNAP.EXE 3.4 - ???
Int 1A/AX=7802h - SNAP.EXE 3.4 - ???
Int 1A/AH=7Fh - Tandy 2500, Tandy 1000L series - DIGITAL SOUND???
Int 1A/AH=80h - PCjr, Tandy 2500???, Tandy 1000SL/TL - SET UP SOUND MULTIPLEXOR
Int 1A/AH=80h - PCMCIA Socket Services v1.00 - GET NUMBER OF ADAPTERS
Int 1A/AH=81h - PCMCIA Socket Services v1.00 - REGISTER STATUS CHANGE CALLBACK
Int 1A/AX=8100h - Tandy 2500, Tandy 1000L series - DIGITAL SOUND - INSTALLATION CHECK
Int 1A/AH=82h - Tandy 2500???, Tandy 1000SL/TL - DIGITAL SOUND - RECORD SOUND
Int 1A/AH=82h - PCMCIA Socket Services v1.00 - REGISTER CARD TECHNOLOGY CALLBACK
Int 1A/AH=83h - Tandy 2500, Tandy 1000L series - START PLAYING DIGITAL SOUND
Int 1A/AH=83h - PCMCIA Socket Services v1.00 - GET SOCKET SERVICES VERSION NUMBER
Int 1A/AH=84h - Tandy 2500, Tandy 1000L series - STOP PLAYING DIGITAL SOUND
Int 1A/AH=84h - PCMCIA Socket Services v1.00 - INQUIRE ADAPTER
Int 1A/AH=85h - Tandy 2500, Tandy 1000L series - DIGITAL SOUND???
Int 1A/AH=85h - PCMCIA Socket Services v1.00 - GET ADAPTER
Int 1A/AH=86h - PCMCIA Socket Services v1.00 - SET ADAPTER
Int 1A/AH=87h - PCMCIA Socket Services v1.00 - INQUIRE WINDOW
Int 1A/AH=88h - PCMCIA Socket Services v1.00 - GET WINDOW
Int 1A/AH=89h - PCMCIA Socket Services v1.00 - SET WINDOW
Int 1A/AH=8Ah - PCMCIA Socket Services v1.00 - GET PAGE
Int 1A/AH=8Bh - PCMCIA Socket Services v1.00 - SET PAGE
Int 1A/AH=8Ch - PCMCIA Socket Services v1.00 - INQUIRE SOCKET
Int 1A/AH=8Dh - PCMCIA Socket Services v1.00 - GET SOCKET
Int 1A/AH=8Eh - PCMCIA Socket Services v1.00 - SET SOCKET
Int 1A/AH=8Fh - PCMCIA Socket Services v1.00 - GET CARD
Int 1A/AH=90h - PCMCIA Socket Services v1.00 - RESET CARD
Int 1A/AH=91h - PCMCIA Socket Services v1.00 - READ ONE
Int 1A/AH=92h - PCMCIA Socket Services v1.00 - WRITE ONE
Int 1A/AH=93h - PCMCIA Socket Services v1.00 - READ MULTIPLE
Int 1A/AH=94h - PCMCIA Socket Services v1.00 - WRITE MULTIPLE
Int 1A/AH=95h - PCMCIA Socket Services v1.00 - INQUIRE ERROR DETECTION CODE
Int 1A/AH=96h - PCMCIA Socket Services v1.00 - GET ERROR DETECTION CODE
Int 1A/AH=97h - PCMCIA Socket Services v1.00 - SET ERROR DETECTION CODE
Int 1A/AH=98h - PCMCIA Socket Services v1.00 - START ERROR DETECTION CODE
Int 1A/AH=99h - PCMCIA Socket Services v1.00 - PAUSE ERROR DETECTION CODE
Int 1A/AH=9Ah - PCMCIA Socket Services v1.00 - RESUME ERROR DETECTION CODE
Int 1A/AH=9Bh - PCMCIA Socket Services v1.00 - STOP ERROR DETECTION CODE
Int 1A/AH=9Ch - PCMCIA Socket Services v1.00 - READ ERROR DETECTION CODE
Int 1A/AH=9Dh - PCMCIA Socket Services v2.1??? - GET VENDOR INFO
Int 1A/AH=9Dh - Intel PCMCIA ExCA Card Services - API
Int 1A/AH=9Eh - PCMCIA Socket Services v2.1 - ACKNOWLEDGE INTERRUPT
Int 1A/AH=9Fh - PCMCIA Socket Services v2.1 - GET/SET PRIOR INT 1A HANDLER
Int 1A/AH=A0h - Disk Spool II v2.07+ - INSTALLATION CHECK
Int 1A/AH=A0h - PCMCIA Socket Services v2.1 - GET/SET SOCKET SERVICES ADDRESS
Int 1A/AH=A1h - PCMCIA Socket Services v2.1 - GET ACCESS OFFSETS
Int 1A/AH=A2h - CardBus Socket Services - ACCESS CONFIGURATION SPACE
Int 1A/AH=A4h - CardBus Socket Services - GET BRIDGE WINDOW / WINDOW CAPABILITIES
Int 1A/AH=A5h - CardBus Socket Services - SET BRIDGE WINDOW
Int 1A/AH=ABh - Disk Spool II v1.83 - INSTALLATION CHECK
Int 1A/AH=ACh - Disk Spool II v1.83 - INSTALLATION CHECK
Int 1A/AH=ADh - Disk Spool II v1.83 - FUNCTION CALLS
Int 1A/AH=AEh - PCMCIA Socket Services v2.1 - VENDOR SPECIFIC
Int 1A/AH=AEh - PCMCIA Socket Services v2.1 - API
Int 1A/AH=AFh - PCMCIA v2 Card Services - API
Int 1A/AX=B000h - HP 100LX/200LX - PCMCIA - ???
Int 1A/AX=B001h/CX=4D52h - Microsoft Real-Time Compression Interface (MRCI) - ROM-BASED SERVER
Int 1A/AX=B101h -
Int 1A/AX=B102h - PCI BIOS v2.0c+ - FIND PCI DEVICE
Int 1A/AX=B103h - PCI BIOS v2.0c+ - FIND PCI CLASS CODE
Int 1A/AX=B106h - PCI BIOS v2.0c+ - PCI BUS-SPECIFIC OPERATIONS
Int 1A/AX=B108h - PCI BIOS v2.0c+ - READ CONFIGURATION BYTE
Int 1A/AX=B109h - PCI BIOS v2.0c+ - READ CONFIGURATION WORD
Int 1A/AX=B10Ah - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD
Int 1A/AX=B10Ah/SF=1004h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (VLSI devices)
Int 1A/AX=B10Ah/SF=100Bh - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (National Semicond. device)
Int 1A/AX=B10Ah/SF=1011h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (DEC device)
Int 1A/AX=B10Ah/SF=1022h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (AMD devices)
Int 1A/AX=B10Ah/SF=1042h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (PC Technology devices)
Int 1A/AX=B10Ah/SF=1045h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (OPTi devices)
Int 1A/AX=B10Ah/SF=1066h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (PicoPower devices)
Int 1A/AX=B10Ah/SF=1066h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (Brooktree devices)
Int 1A/AX=B10Ah/SF=1106h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (VIA Technologies devices)
Int 1A/AX=B10Ah/SF=8086h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (Intel devices)
Int 1A/AX=B10Ah/SF=9004h - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (Adaptec devices)
Int 1A/AX=B10Bh - PCI BIOS v2.0c+ - WRITE CONFIGURATION BYTE
Int 1A/AX=B10Ch - PCI BIOS v2.0c+ - WRITE CONFIGURATION WORD
Int 1A/AX=B10Dh - PCI BIOS v2.0c+ - WRITE CONFIGURATION DWORD
Int 1A/AX=B10Eh/BX=0000h - PCI BIOS v2.1+ - GET IRQ ROUTING INFORMATION
Int 1A/AX=B10Fh - PCI BIOS v2.1+ - SET PCI IRQ
Int 1A/AX=B181h - PCI BIOS v2.0c+ - INSTALLATION CHECK (32-bit)
Int 1A/AX=B182h - PCI BIOS v2.0c+ - FIND PCI DEVICE (32-bit)
Int 1A/AX=B183h - PCI BIOS v2.0c+ - FIND PCI CLASS CODE (32-bit)
Int 1A/AX=B186h - PCI BIOS v2.0c+ - PCI BUS-SPECIFIC OPERATIONS (32-bit)
Int 1A/AX=B188h - PCI BIOS v2.0c+ - READ CONFIGURATION BYTE (32-bit)
Int 1A/AX=B189h - PCI BIOS v2.0c+ - READ CONFIGURATION WORD (32-bit)
Int 1A/AX=B18Ah - PCI BIOS v2.0c+ - READ CONFIGURATION DWORD (32-bit)
Int 1A/AX=B18Bh - PCI BIOS v2.0c+ - WRITE CONFIGURATION BYTE (32-bit)
Int 1A/AX=B18Ch - PCI BIOS v2.0c+ - WRITE CONFIGURATION WORD (32-bit)
Int 1A/AX=B18Dh - PCI BIOS v2.0c+ - WRITE CONFIGURATION DWORD (32-bit)
Int 1A/AX=B18Eh/BX=0000h - PCI BIOS v2.1+ - GET IRQ ROUTING INFORMATION (32-bit)
Int 1A/AX=B18Fh - PCI BIOS v2.1+ - SET PCI IRQ (32-bit)
Int 1A/AH=B2h - Reserved For PCI
Int 1A/AH=B3h - Reserved For PCI
Int 1A/AX=B400h - Intel Plug-and-Play AUTO-CONFIGURATION - INSTALLATION CHECK
Int 1A/AX=B401h - Intel Plug-and-Play AUTO-CONFIGURATION - GET DEFAULT CONFIG TABLE
Int 1A/AX=B402h - Intel Plug-and-Play AUTO-CONFIGURATION - COPY AND VERIFY CONFIG TABLE
Int 1A/AX=B403h - Intel Plug-and-Play AUTO-CONFIGURATION - STORE ESCD TABLE IN NVRAM
Int 1A/AX=B404h - Intel Plug-and-Play AUTO-CONFIGURATION - GET AVAILABLE IRQs???
Int 1A/AX=B405h - Intel Plug-and-Play AUTO-CONFIGURATION - GET ???
Int 1A/AX=B406h - Intel Plug-and-Play AUTO-CONFIGURATION - GET PCI IRQ ROUTING TABLE
Int 1A/AX=B407h - Intel Plug-and-Play AUTO-CONFIGURATION - ???
Int 1A/AH=B4h - Intel Plug-and-Play AUTO-CONFIGURATION - 32-BIT API
Int 1A/AH=C0h - Disk Spool II v2.07+ - ALTERNATE INSTALLATION CHECK
Int 1A/AX=CCCCh/BX=CCCCh - DATEFIX - INSTALLATION CHECK
Int 1A/AH=D0h - Disk Spool II v2.07+ - FUNCTION CALLS
Int 1A/AH=E0h - Disk Spool II v4.0x - ENABLE/DISABLE
Int 1A/AH=E1h - Disk Spool II v4.0x - GET STATUS
Int 1A/AX=E11Bh - TheGrab v4.60 - ???
Int 1A/AX=E11Dh - TheGrab v4.60 - INSTALLATION CHECK
Int 1A/AH=E2h - Disk Spool II v4.0x - GET SPOOL FILES
Int 1A/AX=E301h - Disk Spool II v4.0x - GET SPOOL FILE STATUS
Int 1A/AX=E302h - Disk Spool II v4.0x - UPDATE SPOOL FILE
Int 1A/AX=E401h - Disk Spool II v4.0x - SPOOL EXISTING FILE
Int 1A/AX=E402h - Disk Spool II v4.0x - SPOOL EXISTING FILE???
Int 1A/AH=E5h - Emulaser ELSPL.COM - ???
Int 1A/AH=EEh - Disk Spool II v4.05 - ???
Int 1A/AH=F7h - RighTime v1.1 - TEMPORARILY DISABLE
Int 1A/AH=F8h - RighTime v1.1 - ENABLE
Int 1A/AH=FEh - AT&T 6300 - READ TIME AND DATE
Int 1A/AH=FFh - AT&T 6300 - SET TIME AND DATE
Int 1A/AH=FFh - RighTime v1.1 - PERMANENTLY DISABLE
Int 1A/AX=FF00h - SND - INSTALLATION CHECK???
Int 1A/AX=FF01h - SND - PAUSE
Int 1A/AX=FF02h - SND - START SOUND
Int 1A/AX=FF03h - SND - STOP SOUND
Int 1A/AX=FF04h - SND - PLAY MUSIC STRING IN BACKGROUND
Int 1A/AX=FF05h - SND - UNCONDITIONALLY STOP SOUND

| Interrups | Categories | Contents

Shopping | Forum | EMail | Index | Home |

Rate My Photo